Updates

* Eric:
* Lots of troubleshooting (12/7), aiming for data collecting on 12/8
* Fixing setup to be 16cm apart

Not much else

ASTM D790:

* If specimen does not break at 5% strain at 0.1 mm/mm/min with 16;1 ratio, it is best to do ASTM D638, the Tensile test for plastics